**March 13, 2019**

**Introduction of a new method WIAP MEMV metal relax with vibration**

Good day to management

There are two variants for good processing results as an intermediate operation for precise component manufacturing.

The variant glow stress, or variant: **WIAP MEMV metal relax with vibration**. A component has finished mounting the exciter, usually in an hour.

* No scale
* Reduction of freight costs; it is expanded on site
* electricity savings
* An already painted component can be treated MEMV

Component sizes from 10 kg to 200 tonnes possible.

Ideal for:

* **Welded structures of all kinds.**

**Cylinders, rings, flame directed or hydraulically directed shaped pipes. Sheet metal plates of 10 mm or in bundles.**

**aging cast designs artificial. Small cast designs on Mehrfachaufspannvorrichtung and more,**

Here are the links for

[New Releases 2019](https://www.wiap.ch/Inhaltsverzeichnise/WA05%20Einfuehrung,%20Neuheiten,%20MEMV%202019.htm)

[Brochure 2018](https://www.wiap.ch/MEMV%20Prospekt/Prospekt_Fachartikel_12S_DE_r20.pdfhttps:/www.wiap.ch/MEMV%20Prospekt/Prospekt_Fachartikel_12S_DE_r20.pdf)

[Press release in 2018](https://www.technik-und-wissen.ch/detail/metall-entspannen-mit-vibrationen.html)

We can provide the WIAP MEMV process in person or with more information,

We are pleased to hear from you.

Best regards / best regards

**Hanspeter Widmer**

**WIAP AG Ltd SA**

Industriestrasse 48L

CH 4657 Dulliken, Switzerland

Tel. +41 62 752 42 60

*+41 78 797 48 60*

Mail: [*hanspeter@widmers.info*](mailto:hanspeter@widmers.info)

Website: [www.wiap.ch](http://www.wiap.ch/)